C-Index

A B C D E F G H I L M N O P R S T U V W

## C

CBus0 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus0 Mux Control
CBus0 - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - CBus0 Mux Control
CBus0 - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - CBus0 Mux Control
CBus0 - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - CBus0 Mux Control
CBus1 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus1 Mux Control
CBus1 - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - CBus1 Mux Control
CBus1 - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - CBus1 Mux Control
CBus1 - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - CBus1 Mux Control
CBus2 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus2 Mux Control
CBus2 - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - CBus2 Mux Control
CBus2 - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - CBus2 Mux Control
CBus2 - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - CBus2 Mux Control
CBus3 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus3 Mux Control
CBus3 - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - CBus3 Mux Control
CBus3 - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - CBus3 Mux Control
CBus3 - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - CBus3 Mux Control
CBus4 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus4 Mux Control
CBus4 - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - CBus4 Mux Control
CBus4 - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - CBus4 Mux Control
CBus4 - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - CBus4 Mux Control
CBus5 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus5 Mux Control
CBus5 - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - CBus5 Mux Control
CBus6 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus6 Mux Control
CBus6 - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - CBus6 Mux Control
CBus7 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus7 Mux Control
CBus8 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus8 Mux Control
CBus9 - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Hardware Option - CBus9 Mux Control
CHIPTOP_DEBUG_REQUEST - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines
CHIPTOP_DEBUG_SET_CHIPTOP_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines
CHIPTOP_DEBUG_SET_OTP_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines
CHIPTOP_DEBUG_SET_SFR - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines
CHIPTOP_DEBUG_SET_USB_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines
CHIPTOP_DISABLE_BCD_DECTION - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_ENABLE_REMOTE_WAKE_UP - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_ENABLE_SUSPEND_OUT - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_CHIPTOP_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_CLK - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_DESC_STRING - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_MODE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_OTP_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_OTP_TEST_BYTE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_SFR - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_STATUS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_USB_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_USER_DATA_STATUS - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_GET_VERSION - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_RESET - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SELECT_FUNCTION - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_BCD_DECTION_POLARITY - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_CLK - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_CLK30K_TRIM_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_DS_CTL0_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_DS_CTL1_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_DS_CTL2_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_INTERRUPT_LEVEL - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_OSC_TRIM0_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_OSC_TRIM1_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_PHY_ODT_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_PHY_TXCTL_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_REG_TRIM_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_SR_CTL0_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_SET_SR_CTL1_REG - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
CHIPTOP_WRITE_OTP_TEST_BYTE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.CHIPTOP_CMD
cleanRxData() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Device
  Clear inner read buffer
CLK_DIV_128 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_16 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_2 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_256 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_32 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_4 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_512 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_64 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_DIV_8 - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_IDLE_HIGH - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPICPOL
CLK_IDLE_LOW - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPICPOL
CLK_LEADING - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPICPHA
CLK_NONE - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPIClock
CLK_TRAILING - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.FT4222_SPICPHA
close() - Method in class com.ftdi.j2xx.FT_Device
  Closes a device opened with a previous call to `D2xxManager.openByIndex(Context, int, com.ftdi.j2xx.D2xxManager.DriverParameters)`, `D2xxManager.openBySerialNumber(Context, java.lang.String, com.ftdi.j2xx.D2xxManager.DriverParameters)`, `D2xxManager.openByDescription(Context, java.lang.String, com.ftdi.j2xx.D2xxManager.DriverParameters)` or `D2xxManager.openByLocation(Context, int, com.ftdi.j2xx.D2xxManager.DriverParameters)`.
close() - Method in class com.ftdi.j2xx.protocol.FT_Spi_Slave
  Close FTDI SPI Slave protocol device
clrDtr() - Method in class com.ftdi.j2xx.FT_Device
  Allows the DTR modem control line to be manually de-asserted.
clrRts() - Method in class com.ftdi.j2xx.FT_Device
  Allows the RTS modem control line to be manually de-asserted.
com.ftdi.j2xx.ft4222 - package com.ftdi.j2xx.ft4222
com.ftdi.j2xx.interfaces - package com.ftdi.j2xx.interfaces
createDeviceInfoList(Context) - Method in class com.ftdi.j2xx.D2xxManager
  This method builds an internal device information list and returns the number of D2XX devices connected to the system.

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms