E-Index

A B C D E F G H I L M N O P R S T U V W

## E

eepromErase() - Method in class com.ftdi.j2xx.FT_Device
  Erases the device EEPROM.
eepromGetUserAreaSize() - Method in class com.ftdi.j2xx.FT_Device
  Retrieves the amount of additional space available in the device EEPROM.
eepromRead() - Method in class com.ftdi.j2xx.FT_Device
  This method reads the entire device EEPROM and decodes its settings in to fields in a `FT_EEPROM` object. remarks: `FT_EEPROM` : For FT_232A , FT_232B. `FT_EEPROM_2232H` : For FT_2232H. `FT_EEPROM_2232D` : For FT_2232. `FT_EEPROM_4232H` : For FT_4232H. `FT_EEPROM_232R` : For FT_232R. `FT_EEPROM_245R` : For FT_245R. `FT_EEPROM_232H` : For FT_232H. `FT_EEPROM_X` : For FT_X_Series.
eepromReadUserArea(int) - Method in class com.ftdi.j2xx.FT_Device
  Retrieves the contents of the device EEPROM user area.
eepromReadWord(short) - Method in class com.ftdi.j2xx.FT_Device
  This method reads a WORD from the device EEPROM at the specified address.
eepromWrite(FT_EEPROM) - Method in class com.ftdi.j2xx.FT_Device
  This method encodes the settings from a `FT_EEPROM` object and writes them to the device EEPROM. remarks: `FT_EEPROM` : For FT_232A , FT_232B. `FT_EEPROM_2232H` : For FT_2232H. `FT_EEPROM_2232D` : For FT_2232. `FT_EEPROM_4232H` : For FT_4232H. `FT_EEPROM_232R` : For FT_232R. `FT_EEPROM_245R` : For FT_245R. `FT_EEPROM_232H` : For FT_232H. `FT_EEPROM_X` : For FT_X_Series.
eepromWriteUserArea(byte[]) - Method in class com.ftdi.j2xx.FT_Device
  Writes data to the device EEPROM user area.
eepromWriteWord(short, short) - Method in class com.ftdi.j2xx.FT_Device
  This method writes a WORD to the device EEPROM at the specified address.
ExternalOscillator - Variable in class com.ftdi.j2xx.FT_EEPROM_232R
  Hardware Option - External Oscillator Caution: Setting this bit without an external oscillator fitted to your design will render the device unusable.
ExternalOscillator - Variable in class com.ftdi.j2xx.FT_EEPROM_245R
  Hardware Option - External Oscillator Caution: Setting this bit without an external oscillator fitted to your design will render the device unusable.

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms