R-Index

A B C D E F G H I L M N O P R S T U V W

## R

read(int, boolean[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_Gpio
  Read the value from the specified GPIO pin.
read(int, byte[], int, int[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Master
  Read data from the specified I2C slave device with START and STOP conditions.
read(byte[], int, int[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Slave
  Read data from the buffer of I2C slave device.
read(byte[], int, int[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_Spi_Slave
  Get number of bytes in the receive queue.
read(byte[], int, long) - Method in class com.ftdi.j2xx.FT_Device
  This method reads data from the device in to the Java application buffer.
read(byte[], int) - Method in class com.ftdi.j2xx.FT_Device
  This method reads data from the device in to the Java application buffer.
read(byte[]) - Method in class com.ftdi.j2xx.FT_Device
  This method reads data from the device in to the Java application buffer.
read(int, boolean[]) - Method in interface com.ftdi.j2xx.interfaces.Gpio
  Read the value from the specified GPIO pin.
read(int, byte[], int, int[]) - Method in interface com.ftdi.j2xx.interfaces.I2cMaster
  Read data from the specified I2C slave device with START and STOP conditions.
read(byte[], int, int[]) - Method in interface com.ftdi.j2xx.interfaces.I2cSlave
  Read data from the buffer of I2C slave device.
read(byte[], int, int[]) - Method in interface com.ftdi.j2xx.interfaces.SpiSlave
  Get number of bytes in the receive queue.
readBufferFull() - Method in class com.ftdi.j2xx.FT_Device
  This method return if the Rx buffer was full with data, if true, Rx would be pending until the data is read by user.
readEx(int, int, byte[], int, int[]) - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Master
  Read data from the specified I2C slave device with the specified I2C condition.
readEx(int, int, byte[], int, int[]) - Method in interface com.ftdi.j2xx.interfaces.I2cMaster
  Read data from the specified I2C slave device with the specified I2C condition.
registerSpiSlaveListener(SpiSlaveListener) - Method in class com.ftdi.j2xx.protocol.FT_Spi_Slave
  Register SPI Slave action listener
RemoteWakeup - Variable in class com.ftdi.j2xx.FT_EEPROM
  String Descriptor - Remote Wakeup Enabled
Repeated_START - Static variable in class com.ftdi.j2xx.ft4222.FT_4222_Defines.I2C_MasterFlag
RES_SLAVE_READ - Static variable in class com.ftdi.j2xx.protocol.SpiSlaveResponseEvent
  Response type from spi slave processor
reset() - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Master
  Reset the I2C master device.
reset() - Method in class com.ftdi.j2xx.ft4222.FT_4222_I2c_Slave
  Reset the I2C slave device.
reset() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Spi_Master
  Reset the SPI master device.
reset() - Method in class com.ftdi.j2xx.ft4222.FT_4222_Spi_Slave
  Reset the SPI slave device.
reset() - Method in interface com.ftdi.j2xx.interfaces.I2cMaster
  Reset the I2C master device.
reset() - Method in interface com.ftdi.j2xx.interfaces.I2cSlave
  Reset the I2C slave device.
reset() - Method in interface com.ftdi.j2xx.interfaces.SpiMaster
  Reset the SPI master device.
reset() - Method in interface com.ftdi.j2xx.interfaces.SpiSlave
  Reset the SPI slave device.
RESET - Static variable in class com.ftdi.j2xx.protocol.SpiSlaveResponseEvent
  Response code from spi slave processor
resetDevice() - Method in class com.ftdi.j2xx.FT_Device
  This method sends a vendor command to the device to cause a reset and flush any data from the device buffers.
restartInTask() - Method in class com.ftdi.j2xx.FT_Device
  Restarts the driver's IN thread following a successful call to `FT_Device.stopInTask()` Remarks: This function is used to restart the driver's IN task (read) after it has been stopped by a call to `FT_Device.stopInTask()`.
RS485EchoSuppress - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Hardware Option - RS485 Echo Suppression

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms