A-Index

A B C D E F G H I L M N O P R S T U V W

## A

A_DeviceTypeValue - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
A_FastSerial - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Hardware Option - Interface A Fast Serial
A_FastSerial - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface A Fast Serial
A_FIFO - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Hardware Option - Interface A 245 FIFO
A_FIFO - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface A 245 FIFO
A_FIFOTarget - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Hardware Option - Interface A 245 FIFO CPU Target
A_FIFOTarget - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface A 245 FIFO CPU Target
A_HighIO - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Drive Option - Interface A High Current IO
A_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Driver Option - Interface A Load D2XX
A_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Driver Option - Interface A Load D2XX Port
A_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Driver Option - Load D2XX
A_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Driver Option - Interface A Load Vitrual Com Port
A_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Driver Option - Interface A Load virtual Com Port
A_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Driver Option - Load Virtual Com Port
A_UART - Variable in class com.ftdi.j2xx.FT_EEPROM_2232D
  Drive Option - Interface A UART
A_UART - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Hardware Option - Interface A 245 UART
AC_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Drive Option - AC pins drive current.
AC_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Drive Option - AC pins have Schmitt input.
AC_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Drive Option - AC pins have slow slew.
AD_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Drive Option - AD pins drive current.
AD_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Drive Option - AD pins have Schmitt input.
AD_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_X_Series
  Drive Option - AD pins have slow slew.
addUsbDevice(UsbDevice) - Method in class com.ftdi.j2xx.D2xxManager
  This method analyze the dev passed-in, if it's a FTDI device, add it to manageable device list
AH_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - AH pins have driver current.
AH_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - AH pins drive current.
AH_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface AH Load D2XX
AH_LoadRI_RS485 - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface AH Load RI_RS485
AH_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface AH Load Vitrual Com Port
AH_RI_TXDEN - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Hardware Option - Interface AH uses RI as RS485 TXDEN
AH_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - AH pins have schmitt input.
AH_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - AH pins have Schmitt input.
AH_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - AH pins have slow slew.
AH_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - AH pins have slow slew.
AL_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - AL pins have driver current.
AL_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Drive Option - AL pins drive current.
AL_DriveCurrent - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - AL pins drive current.
AL_LoadD2XX - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface AL Load D2XX
AL_LoadRI_RS485 - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface AL Load RI_RS485
AL_LoadVCP - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Driver Option - Interface AL Load Vitrual Com Port
AL_RI_TXDEN - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Hardware Option - Interface AL uses RI as RS485 TXDEN
AL_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - AL pins have schmitt input.
AL_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Drive Option - AL pins have Schmitt input.
AL_SchmittInput - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - AL pins have Schmitt input.
AL_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_2232H
  Drive Option - AL pins have slow slew.
AL_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_232H
  Drive Option - AL pins have slow slew.
AL_SlowSlew - Variable in class com.ftdi.j2xx.FT_EEPROM_4232H
  Drive Option - AL pins have slow slew.

A B C D E F G H I L M N O P R S T U V W

About FTDI | FTDI Licence Terms